IMPORTANT: READ ME

USE AT YOUR OWN RISK

THIS CONFIGURATION IS BASED ON SENSORLESS HOMING
Meaning it is setup to NOT use the standard END-STOPS. 
Disconnect X and Y Endstop when using this zip file.

Use:
Copy all the folders including the bin file to the root of the SD card,

\\SD CARD
\filaments\
\gcodes\
\macros\
\menu\
\sys\
\www\
Firmware.bin

Folder: filaments
 contains Sub-Folders with specific unload and Load files for each type of filament.
Folder: gcodes
 contains your g-code files for printing
Folder: macros
 contains macro files, which are just filename.g files where you can create a sequence of gcode commands to be performed.
Folder: menu
 contains the files needed to use the Standard 12864 display
Folder: sys
 contains the configuration files for you printer, easy to modify from the DWC
Folder: www
 contains the files for the DWC. (Web interface)
 
firmware.bin is in the root of the SD Card. 

 IMPORTANT: DO THIS:
 open de sys folder and modify the "runonce.g"
 this file will be used once, so we use it to setup the Wifi connection and have the firmware files installed at first starting of the printer.